

**SOUTHERN AFRICAN DEVELOPMENT COMMUNITY.**

**TENDER DOCUMENT**

**Supply and Installation of SPGRC Palisade Boundary Fence in Lusaka, Zambia**

**TENDER NO: *In Situ 03/2023-24***

**Number of Lots:** 1

**Version 1.1**

**SOUTHERN AFRICAN DEVELOPMENT COMMUNITY SECRETARIAT,**

**PLOT 54385 CBD**

**P / BAG 0095**

**GABORONE**

**BOTSWANA**

**November 2023**

|  |  |
| --- | --- |
|  |  |

TENDER DOCUMENT (TD) – SUPPLY AND INSTALLATION OF SPGRC PALISADE BOUNDARY FENCE IN LUSAKA, ZAMBIA

|  |  |
| --- | --- |
| **Supply and Installation of SPGRC Palisade Boundary Fence in Lusaka, Zambia** | DATE: 13th November 2023 |
| REFERENCE: ***In Situ 03/2023-24*** |

Dear Sir / Madam:

We kindly request you to submit your quotation for undertaking the **Supply and Installation of SPGRC Palisade Boundary Fence in Lusaka, Zambia** as detailed in item 2 of this TD. When preparing your quotation, please be guided by the Bill of Quantities attached hereto as Annex A and Annex B.

Quotations may be submitted at or before Mid night Zambia local time **13th December 2023**  and to the following link below:

<https://collab.sadc.int/s/HKme9KoBa86P9xr>

Quoting the reference below:

**TD # *In Situ 03/2023-24***

**Supply and Installation of SPGRC Palisade Boundary Fence in Lusaka, Zambia**

It shall remain your responsibility to ensure that your quotation will reach the address above on or before the deadline. Quotations that are received by SPGRC after the deadline indicated above, for whatever reason, shall not be considered for evaluation. You shall return this document together with the required documents as they would form the Contract Documents.

**There shall be a compulsory site visit on 17 November 2023, at 10:00 hours, at the SPGRC Premises in Chongwe. Please note that tenderers who fail to send a representative to this compulsory site visit will automatically be disqualified. Tenderers who arrive after 10:00 hours will not be allowed in the Site Visit meeting.**

For any further clarifications, please send them to the following email:[**spgrc@sadc.int**](mailto:tenders@sadc.int) **;**[**tamarap@sadc.int**](mailto:frandrianiaina@sadc.int) **and** [**phirit@sadc.int**](mailto:mmalongo@sadc.int) **and copy to** [**tchabwera@sadc.int**](mailto:tchabwera@sadc.int)[**DO NOT USE THESE EMAILS FOR SUBMISSION OF YOUR OFFERS]. Offers submitted as hard copies will be rejected.**

**EXPLANATIONS CONCERNING BIDDING DOCUMENTS**

**Bidders may submit questions in writing up to 22nd November 2023 at 1700hrs, specifying the publication reference and the contract title:**

**The Contracting Authority has no obligation to provide additional information after this date.**

**The Contracting Authority will reply to all bidders’ questions, latest by 28th November 2023 at 1700hrs.**

Yours Sincerely

Dr.Justify Shava

**Head of SPGRC**

**1: BACKGROUND INFORMATION**

1. At its premises in Chongwe, Zambia, SPGRC, has a stretch of its boundary fence which is prone to damage and intrusion by trespassers. This poses a risk to the SPGRC assets within the premises. SPGRC intends to erect a solid barrier along this stretch which is estimated to be 0.5km to offer permanent solution to trespassing and vandalism along this stretch of the boundary fence.
2. For this purpose, SPGRC intends to appoint a company for undertaking the SPGRC 500m Palisade Boundary Fence in Lusaka, Zambia (hereinafter referred to as the “**Project**”), as detailed in this TD and in this connection invites quotations from the Bidders for carrying out / executing the Project.

Quotations, electronic copies only, may be submitted in PDF Format via the COLLAB link below below:

[**https://collab.sadc.int/s/HKme9KoBa86P9xr**](https://collab.sadc.int/s/HKme9KoBa86P9xr)

**The reference for the tender is:**

**TD # *In Situ 03/2023-24***

**Supply and Installation of SPGRC Palisade Boundary Fence in Lusaka, Zambia**

**Person responsible for any additional information and receipt of proposals:**

Ms Tamara Phiri

Assistant Administration Officer

E-Mail: [tamarap@sadc.int](mailto:vchingalawa@sadc.int)

**2. PROJECT SCOPE**

The following is the scope and extent of work to be covered in this project.

2.1 Lot 1 -To undertake the Supply and Installation of SPGRC 500m Palisade Boundary Fence in Lusaka, Zambia as detailed in the Bills of Quantities, Annex A.

Other deliverables:

1. Conduct all the necessary tests and commissioning as per the government specifications
2. The contractor will be responsible for obtaining all the approvals and certificates from relevant authorities as necessary
3. All work will comply with internationally acceptable standards, statutory and local government requirements.
4. The works shall comply with the applicable statutory regulations to avoid infringing with existing laws, regulations, practices and standards.
5. The contractor will provide a level of supervision that will ensure that work is carried out according to design, specifications and programme.
6. The contractor shall attend to all defects during defects liability period.
7. The contractor may submit the proposals for any other services that he feels may be appropriate for a project of this nature for the client’s consideration.

**3: PROJECT SPECIFIC CONDITIONS**

Please take note of the following requirements and conditions pertaining to this project.

|  |  |
| --- | --- |
| Tender Submission COLLAB link | [**https://collab.sadc.int/s/HKme9KoBa86P9xr**](https://collab.sadc.int/s/HKme9KoBa86P9xr)  **Reference:**  **TD # *In Situ 03/2023-24***  **Supply and Installation of SPGRC 500m Palisade Boundary Fence in Lusaka, Zambia** |
| Method of TD Submission | Electronic in PDF Format via the COLLAB link below  [**https://collab.sadc.int/s/HKme9KoBa86P9xr**](https://collab.sadc.int/s/HKme9KoBa86P9xr)  **Reference:**  **TD # *In Situ 03/2023-24***  **Supply and Installation of SPGRC Palisade Boundary Fence in Lusaka, Zambia**  **Tender submission is electronic only** |
| Compliance to tender | The following shall constitute compliance to tender:   * Certificate of incorporation / Company registration certificate * Compulsory Site Visit * Valid Tax Clearance Certificate * Sworn Statement (To be sworn under Oath Commissioner or Notary) * Duly completed Directors and Shareholders Declaration Form * Vat Certificate or Exemption Certificate only where applicable * Power of Attorney (To be sworn under Oath Commissioner or Notary) * **AUTHORISED SIGNATORIES MUST INITIAL ON EACH PAGE OF THE SUBMITTED BID DOCUMENT FAILURE TO DO THIS WILL RESULT IN AUTOMATIC DISQUALIFICATION.** |
| Date of Distribution of Tender Document | 13th November 2023 |
| Type of Bidding | Negotiated Procedure |
| Compulsory Site Visit | 17 November 2023 |
| Submission Deadline Date and time | 13th December 2023 |
| Bid Opening | 14 December 2023 at 10:00 hours. |
| Planned Tender Evaluation | December 2023 |
| Planned Tender Award | January 2024 |
| Validity of Quotation | Ninety (90) days |
| Time to complete project | To be proposed by Bidder |
| Currency of Quotation | Zambia Kwacha |
| Payment Terms | Full payment after completion of the work |
| Time within which payment to be made after receipt of contractors’ certificate. | Thirty (30) calendar days after submission of undisputed claim for measured and valued work. |
| Form of Contract | SADC Standard Contract For Construction Works |
| Commencement of work | Not exceeding 5 days after contract signing |
| **Type of Contract** | **Fixed Price Contract.**  **Purchase order to be issued to the winning bidder** |

**4. EVALUATION OF TENDERS**

**4.1 SPGRC Tender Evaluation**

The evaluation of tenders will be conducted by at least three (3) SPGRC officials appointed by the Head of SPGRC.

**4.2 SPGRC Tender Evaluation Stages**

Evaluation shall be carried out in three (3) stages. In stage one (1), tenders shall be checked to ensure that the bids are submitted in accordance with Compliance with the above stated requirements. Those bids that do not meet the requirements will be considered “non-compliant” and shall be disqualified.

In stage two (2) tenders that are fully compliant shall have their Technical proposals evaluated for compliance to the requirements in Table 4.4 below and lastly those Technically Compliant evaluated at Financial Stage.(Those which got YES in all the TECHNICAL VARIABLES)

**4.4 Technical Tender Evaluation Criteria**

Table 4.4

|  |  |  |  |
| --- | --- | --- | --- |
| **Evaluation Area** | **Item Description** | **Compliant/Non-Compliant YES/NO** | **Comments** |
|  |  |  |  |
|  |  |  |
| Methodology & work plan | Technical content of the methodology |  |  |
|  | Project programme & work plan |  |
| Qualification and Experience of proposed key technical staff | Bachelors Degree in Engineering or Equivalent with 3 years Qualification and experience of the proposed key expert who will undertake the work |  |  |
| Firm’s Project Reference | Experience of the company in undertaking projects of similar nature. List and elaborate all similar project(Fencing)of at least $50,000 from three (3) cumulative contracts done in the past five (5) years Provide at least three (3) contactable references of similar works done previously, Submit Purchase Orders for the projects of similar nature as stated above. |  |  |
| Quality Assurance | Elaborate any quality assurance initiatives to be undertaken when executing the project. |  |  |
|  |  |  |  |

|  |
| --- |
|  |

**4.5 Award Criteria**

The award will be to the bidder submitting the least expensive TECHNICALLY COMPLIANT BID and to the one with ALL items below QUOTED FOR and as such failure to quote for all items in a lot in the Bill of Quantities below will lead to Automatic Disqualification. If a Price Schedule shows items listed but not priced, their prices shall be assumed to be included in the prices of other items. An item not listed in the Price Schedule shall be assumed to be not included in the bid

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **PRELIMINARIES AND GENERAL ITEMS** |  | | |  |  |
| **ITEM** | **DESCRIPTION** | **UNIT** | **QTY** | **RATE** | **AMOUNT** |  |
| A | Contractor's Mobilisation | Item | 1 |  |  |  |
| B | Site Meeting | Item | 1 |  |  |  |
| C | Person-in-charge | Item | 1 |  |  |  |
| D | Plant, Tools, Vehicles, and Scaffolding | Item | 1 |  |  |  |
| E | Site Administration and Security | Item | 1 |  |  |  |
| F | Transport for Work people | Item | 1 |  |  |  |
| G | Temporary Accommodation for use of the Contractor | Item | 1 |  |  |  |
| H | Safety, Health and Welfare of Work People  **PRELIMINARIES AND GENERAL ITEMS TOTAL -** | Item | 1 |  |  |  |
|  | **CARRIED TO GENERAL SUMMARY** |  |  |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ITEM** | **DESCRIPTION** | **QTY** | **UNIT** | **RATE** | **AMOUNT** |
|  | **DEMOLITIONS (ALL PROVISIONAL)** |  |  |  |  |
|  | Notes on demolitions |  |  |  |  |
|  | The contractor shall be deemed to have visited the site to familiarise themselves with the works measured under this section and no extra claims shall be entertained arising from inadequate and /or lack of understanding of the nature, magnitude and scope of works measured here under |  |  |  |  |
|  | Demolitions and down takings |  |  |  |  |
| A | Take down existing boundary barbed wire fence and, handover to client and remove debri from the site | item | 1 |  | - |
|  | **Demolitions Total Carried to Summary** |  |  | **K** | **-** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ITEM** | **DESCRIPTION** | **QTY** | **UNIT** | **RATE** | **AMOUNT** |
| A  B  C  D  E  F  G  H  J  K  L  M N | **BOUNDARY PALISADE BOUNDARY FENCE**  The following in wall and palisade boundary fence as described  **Excavation works**  Excavate over site average 150 mm deep to remove top soil and wheel, spread and level on site where directed.  Excavate for foundation trenches not exceeding 1.50metres deep, get out, part back fill and spread on site any surplus material as described  Extra over excavations for excavating in hard rock  **Concrete works**  Vibrated in situ concrete Grade 25 (20mm aggregate) as described in strip foundation  Vibrated in situ concrete Grade 25 (20mm aggregate) as described in isolated pads  **Blockwork**  Lay150mm solid concrete blocks foundation walls, with cement mortar of ratio 1:4,notmorethan1metreheightblockworkfrom footing  Construct 150mm solid concrete block column size 400mm x 400mm x 2500m high from concrete pad, with cement mortar of ratio 1:4;  Lay 150 mm concrete blocks superstructure walls, with cement mortar of ratio 1:4- Area of blockwork for superstructure  Brick force reinforcement to wall joints every third course width 100mm end laps minimum 100mm wide  Pre-cast concrete (1:2: 4 - 20 mm aggregate as described, including all formwork, moulds, reinforcement, reinforcement for handling, hoisting in position, building in and bedding and pointing in cement mortar 1:4 as described  Concretecoping280mmx115mm(average) deep and bedding as described  Concretecoping500mmx115mm(average)deepandbeddingas described  **Wall Finishings**  One coat wooden trowel finish cement sand (1:4) plaster: 15mm to dwarf walls  15mm to block column externally  Carried Forward | 200  240  24  60  16  250  126  250  1,000  500  63  500  373 | m²  m³  m³  m³  m³  m²  nr  m²  m  m  m  m²m² |  | -  -  -  -  -  -  -  -  -  -  -  -  - |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **ITEM** | **DESCRIPTION** | **QTY** | **UNIT** | **RATE** | **AMOUNT** |
| A  B | Brought Forward  **Painting and decorations**  Plascon or equal and approved sealing coat, three coats Acrylic PVA paint as described to:  Plastered walls and columns  **Palisade Fencing**  Palisade fence consisting of 75 x75mm square hollow tube framing,30x30mmsteelanglesspacedat150mmcentres sharpenedatthetopendand2no.50x50mmsquaresteel horizontal member anchored to block column with rawl bolts  **BOUNDARY FENCE -TOTALCARRIED TO GENERAL SUMMARY** |  |  |  | - |
| 873 | m² |  | - |
| 810 | m² |  | - |
|  |  | **K** | **-** |

|  |  |  |  |
| --- | --- | --- | --- |
| **ITEM** | **DESCRIPTION** | **PAGE** | **AMOUNT (ZMW)** |
| AB C | **MAIN SUMMARY** |  |  |
| PRELIMINARY AND GENERAL ITEMS |  | - |
| DEMOLITIONS |  | - |
| PALISADE BOUNDARY FENCE |  | - |
| **SUBTOTAL 1** |  | **-** |
| ADD 5% CONTIGENCY |  | - |
| **SUBTOTAL 2** |  | **-** |
| ADD 16% VAT |  | - |
| **TOTAL TENDER SUM** |  | **-** |
| **Name of Contractor:** |  |  |
| **Address:** |  |
|  | **Signature:** |  |
| **Date:** |  |

**NB: All bidders have to mandatory visit the site on 17 November 2023 at 10:00 hours for them to qualify for bidding.**

**ALL goods used for these works must be new and unused**

1. **Acceptance of Tender**

SADC is not bound to accept the lowest or any proposal it receives and will not assign reasons for non-acceptance thereof. The cost of preparation and submission of tender documents is the responsibility of the contractor

**5. SITE VISIT**

**All bidders are requested to attend a site visit on 17 November 2023 at 10:00hrs. You are all requested to meet at the SPGRC Office Complex Main Gate at Plot No. 6300 Off Great East Road Chongwe, Zambia before proceeding to the actual site of the project. Tenderers who arrive after 10:00hrs will not be allowed into the meeting.**

**The Contact Person is Ms Tamara Phiri: Contact Number +260 211 399 200**

**AnneX a**

**TERMS OF REFERENCE (TORs) FOR THE CONSTRUCTION OF A PALISADE BOUNDARY FENCE FOR SADC PLANT GENETIC RESOURCES CENTRE**

The contractor shall be deemed to have visited the site to familiarize themselves with the works measured under this section and no extra claims shall be entertained arising from inadequate and /or lack of understanding of the nature, magnitude and scope of works measured here under.

**ANNEX. C**

**POWER OF ATTORNEY**

Please attach here the power of attorney empowering the signatory of the bid and all related documentation.

Signature: ..................................................................................

(*a person or persons authorised to sign on behalf of the bidder*)

Date: .....................

***TEMPLATE OF THE SWORN STATEMENT***

*To be submitted on the headed notepaper of the legal entity concerned*

*<Date>*

*To: Head of SPGRC*

*SADC Plant Genetic Resources Centre*

*Private Bag CH6*

*Lusaka, Zambia*

*Your ref:* **In Situ 03/2023-24**

*Dear Sir/Madam*

*In response to your prequalification notice < Publication reference >, we, < Name(s) of legal entity or entities>,*

*hereby declare that we do not fall into any of the following situations:*

*• being bankrupt or wound up, are having our affairs administered by the courts, have entered into arrangements with creditors, have suspended business activities, are being subject of proceedings concerning those matters, or are being in any similar situations arising from a similar procedure provided for in the national legislation or regulations of the SADC member states.*

*• have been convicted of offences concerning our professional conduct by a judgment, which has the force of res judicata; (i.e. against which no appeal is possible).*

*• have been declared guilty of grave professional misconduct proven by any means which Procuring Entity can justify.*

*• have been the subject of a judgment which has the force of res judicata for fraud, corruption, involvement in a criminal organisation or any other illegal activity detrimental to the Procuring Entity' financial interests.*

*• are being currently subject to an administrative penalty.*

*We further declare that in case we get shortlisted we will provide necessary supporting documents that will prove that we do not fall into any of*

**Annex D**

**Contract SAMPLE ONLY Template**

****

**STANDARD CONTRACT**

**For**

**WORKS**

**Contract Number: *In Situ 03/2023-24***

**………………………………………………………………………………………………..**

**SUPPLY AND INSTALLATION OF A PALISADE BOUNDARY FENCE IN LUSAKA, ZAMBIA**

Between

**SADC Plant Genetic Resources Centre (SPGRC)**

(‘The Contracting Authority’),

And

***…………………………………***

(‘the Contractor’)

**June 2023**

**FORM OF CONTRACT**

This CONTRACT (hereinafter called the “Contract”) is made this *\_\_\_\_\_\_\_\_\_\_* day of the ……………………………..,

Between,

***SADC Secretariat of Gaborone, Botswana, through the SADC Plant Genetic Resources Centre (SPGRC)*, a UNIT of the SADC Secretariat *or corporation incorporated under the***

***laws of Zambia***having its principal place of business **Plot No. 6300 Off Great East Road Chalimbana Research Station, Chongwe**, Zambia (hereinafter referred to as the “Contracting Authority”), on the one hand,

And

***…………………………………………………………………………………………………………………………………………………………………………………………………*** (hereinafter referred to as the “Contractor”), on the other hand,

**WHEREAS** the Contracting Authority desires to have the Works namely the Supply and Installation of SPGRC boundary fence, in Lusaka, Zambiafor ***SADC Plant Genetic Resources Centre (SPGRC)***, Lusaka , Zambia as enumerated and referred to in the General Conditions of Contract, Scope of works , Priced Bills of Quantities and Specifications , Conditions of Particular Application , Contractor’s Tender , award letter, acceptance to award of contract , and any other relevant correspondence executed and completed;

**AND WHEREAS** the Contracting Authority has accepted a tender by the Contractor for the execution and completion of such Works and the remedying of any defects therein.

**It is hereby agreed as follows:**

(1) In this Contract, words and expressions shall have the meanings assigned to them in the contractual conditions set out below.

(2) The following documents shall be deemed to form and be read and construed as part of this Contract, in the following order of precedence:

1. Performance Security Form (Annexure A),
2. Terms of Reference - Lot 1(Annexure B),
3. Contractor’s Bid and Original Price Schedules (Annexure D),
4. Notification of Contract Award (Annexure E),
5. Acceptance to Award of Contract (Annexure F),

The various documents making up the Contract shall be deemed to be mutually explanatory; in cases of ambiguity or divergence, they shall prevail in the order in which they appear above. Any addenda shall have the order of precedence of the document they are amending.

(3) In consideration of the payments to be made by the Contracting Authority to the Contractor as hereinafter mentioned, the Contractor undertakes to execute and complete the Works namely the Supply and Installation of SPGRC Solar Street Lights in Lusaka, Zambia and remedying of defects therein in full compliance with the provisions of this Contract.

(4) The general conditions governing the Contract shall be SADC Standard Contract for Construction works

1. ***Period of execution of Works***
2. The Contractor shall execute and complete the Works within the period of--------------months from the date of commencement of Works as indicated in writing by the Project Manager.
3. Notwithstanding the provision of Clause 4(i) of this Contract, the Project Manager may extend the period of execution of Works if, upon request by the Contractor, he is of considered opinion that the execution of Works was delayed by obstructions, conditions or other circumstances that made it difficult for the Contractor to timely execute the Works.
4. ***Execution of Works***

(i) The Contractor shall:

1. ***Payments***
2. The Contracting Authority hereby agrees to pay the Contractor in consideration of the execution and completion of the Works and remedying of defects therein the amount of **…………………………………………** as fixed price.
3. Payments shall be made in accordance with the certificate approved by the Project Manager.
4. Full payment to be made after completion of the work
5. Payment shall be made to the Contractor in Zambia Kwacha and, where applicable, VAT shall be payable on such sums at the applicable rate. The Contractor must, where applicable in all cases, provide his VAT registration number on all invoices.
6. Payments shall be based on invoice submitted to the Contracting Authority and shall be paid within 30 days of receipt and approval of the of the invoice by the Contracting Authority’s Project Manager, and subject to the Contractor having complied with its obligations hereunder in full as stated in this Contract.
7. The Contracting Authority reserves the right to delay and/or withhold, fully or partially, payments that have not been supported by full and appropriate supporting evidence that the services provided were delivered and accepted by the Contracting Authority.
8. Notwithstanding the provisions of this Sub-clause (c), failure by the Contracting Authority to make payment claimed by the Contractor under this Contract shall not entitle the Contractor to terminate this Contract if such payment has been withheld, delayed, or disapproved by the Contracting Authority due to unsatisfactory work done, or unacceptable invoice submitted, by the Contractor.
9. ***Project Manager***

The Contracting Authority appoints the Project Manager Ms Tamara Phiri to be its Project Manager for the purposes of this Contract.

1. ***Liquidated Damages***

Except where an extension is granted pursuant to Clause 4 (a) (ii) above, if the Contractor fails to complete the Works in accordance with the Works Order from the Project Manager or before the Provisional Completion Date, the Contracting Authority shall levy liquidated damages at 0.5% of the Contract Price for each month of delay; limited to a maximum of 5% of Contract Price.

1. ***Retention Money***

An amount equivalent to 5% (five percent) of the certified gross value of Works done will be deducted and held by the Contracting Authority as Retention Money. 100% of Retention Money shall be released upon issue of Completion Certificate, after the Defects Liability Period; provided that the Works are free from defects and the Contractor has rectified all defects identified by the Contracting Authority and subject to the submission by the Contractor of approvals by the Contracting Authority.

1. ***Defect Rectification / Liability period***

The defect rectification/liability period shall be twelve (12) months from issuance of the Practical Completion Certificate and subsequent handing over of the same to the Contracting Authority.

1. ***Dispute Resolution and applicable law:***
2. The Parties shall use all their best efforts to settle all disputes arising out of, or in connection with, this Contract or its interpretation amicably.
3. In the event that, through negotiation, the parties fail to solve a dispute arising from the conclusion, interpretation, implementation or termination of this Contract, the Parties shall settle the dispute by arbitration.
4. The arbitral tribunal shall consist of three arbitrators. Each party to the dispute shall appoint one arbitrator. The two arbitrators so appointed shall appoint the third arbitrator, who shall be the Chairperson. If within 15 days of receipt of the request for arbitration either party has not appointed an arbitrator, or within 7 days of the appointment of the arbitrators the third arbitrator has not been appointed, either party may request an appointing authority agreed by the parties to appoint an arbitrator.
5. If no appointing authority has been agreed upon by the parties, or if the appointing authority agreed upon refuses to act or fails to appoint the arbitrator within sixty days of the receipt of a party’s request therefore, either party may request the Institute of Arbitrators, Zimbabwe to appoint the third arbitrator.
6. The appointing authority shall, at the request of one of the parties, appoint the sole arbitrator as promptly as possible.
7. The procedure of arbitration shall be fixed by the arbitral tribunal which shall have full power to settle all questions of procedure in any case of disagreement with respect thereto.
8. The decisions of the arbitral tribunal shall be final and binding upon the parties.
9. The arbitration shall take place in Botswana and substantive law of Botswana shall apply.

|  |  |
| --- | --- |
| ***(j)*** | **Termination of Contract** |
| ***(i)*** | *By ContractingAuthority*  The Contracting Authority may terminate this Contract in case of the occurrence of any of the events specified in paragraphs (a) through (g) below. In such an occurrence the Contracting Authority shall give a not less than fifteen (15) days’ written notice of termination to the Contractor, and fifteen (15) days’ also in case of the event referred to in (g).  (a) If the Contractor fails to remedy a failure in the performance of its obligations hereunder, as per served notice, within fifteen (15) days of receipt of such notice or within such further period as the Contracting Authority may have subsequently approved in writing.  (b) If the Contractor becomes (or, if the Contractor consists of more than one entity, if any of its Members becomes) insolvent or bankrupt or enter into any agreements with their creditors for relief of debt or take advantage of any law for the benefit of debtors or go into liquidation or receivership whether compulsory or voluntary.  (c) If the Contractor fails to comply with any final decision reached as a result of arbitration proceedings.  (d) If the Contractor, in the judgment of the Contracting Authority, has engaged in corrupt or fraudulent practices in competing for or in executing this Contract.  (e) If the Contractor submits to the Contracting Authority a false statement which has a material effect on the rights, obligations or interests of the Contracting Authority.  (f) If, as the result of Force Majeure, the Contractor is unable to perform a material portion of the Services for a period of not less than fifteen (15) days.  (g) If the Contracting Authority, in its sole discretion and for any reason whatsoever, decides to terminate this Contract. |
| **(ii)** | **By the Contractor**  The Contractor may terminate this Contract, by not less than thirty (30) days’ written notice to the Contracting Authority, in case of the occurrence of any of the events specified above (a) through (d).  (a) If, as the result of Force Majeure, the Contractor is unable to perform a material portion of the Services for a period of not less than fifteen (15) days. |

1. **Insurance/Injuries**
2. The Contractor has sole responsibility and liability under this Agreement for bodily injuries to Contractor or Contractor’s employees, including responsibility to provide appropriate workers compensation insurance. Contractor hereby warrants to SADC that Contractor is in compliance with any applicable worker’s compensation insurance law.
3. The Contractor has sole responsibility to obtain any other desired insurance coverage (liability, medical, travel, life, etc.) for Contractor and Contractor’s employees in performing this Agreement. 5.3 Neither Contractor nor Contractor’s employees shall be deemed employees of SADC for any purposes, nor shall they participate in any SADC employee benefit or insurance programs.
4. **Privileges and Immunities**

Nothing in or relating to this Contract will be deemed as a waiver, express or implied, of any of the privileges and immunities of SADC.

(5) This Contract shall take effect on the date on the last signature.

(6) Except by mutual agreement in writing between the parties, no modification or amendment shall be made to the present Contract.

**IN WITNESS WHEREOF**, we the undersigned, being duly authorized, have signed this Agreement, in four (4) originals in the English language all copies being equally authentic.

|  |  |  |  |
| --- | --- | --- | --- |
| **For the Contractor** | | **For the Contracting Authority** | |
| Name: |  | Name: |
| Title: |  | Title: |
| Signature |  | Signature: |
| Date:  Place: |  | Date:  Place: |

**ANNEXURE B: TERMS OF REFERENCE**

**TERMS OF REFERENCE**

**ERECTING OF A BOUNDARY FENCE AT THE SADC PLANT GENETIC RESOURCES CENTRE SPGRC**

The contractor shall be deemed to have visited the site to familiarize themselves with the works measured under this section and no extra claims shall be entertained arising from inadequate and /or lack of understanding of the nature, magnitude and scope of works measured here under.

|  |  |
| --- | --- |
| **K** | **AMOUNT**  -  -  -  -  -  -  -  -  **-** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | PRELIMINARIES AND GENERAL ITEMS |  | | |
| ITEM | DESCRIPTION | UNIT | QTY | RATE |
| A | Contractor's Mobilisation | Item | 1 |  |
| B | Site Meeting | Item | 1 |  |
| C | Person-in-charge | Item | 1 |  |
| D | Plant, Tools, Vehicles, and Scaffolding | Item | 1 |  |
| E | Site Administration and Security | Item | 1 |  |
| F | Transport for Work people | Item | 1 |  |
| G | Temporary Accommodation for use of the Contractor | Item | 1 |  |
| H | Safety, Health and Welfare of Work People  PRELIMINARIES AND GENERAL ITEMS TOTAL - | Item | 1 |  |
|  | CARRIED TO GENERAL SUMMARY |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ITEM | DESCRIPTION | QTY | UNIT | RATE | AMOUNT |
|  | DEMOLITIONS (ALL PROVISIONAL) |  |  |  |  |
|  | Notes on demolitions |  |  |  |  |
|  | The contractor shall be deemed to have visited the site to familiarise themselves with the works measured under this section and no extra claims shall be entertained arising from inadequate and /or lack of understanding of the nature, magnitude and scope of works measured here under |  |  |  |  |
|  | Demolitions and down takings |  |  |  |  |
| A | Takedownexistingboundarybarbedwirefenceapproximately2m highand500mlong,handovertoclientandremovedebrifrom | item | 1 |  | - |
|  | Demolitions Total Carried to Summary |  |  | K | - |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ITEM | DESCRIPTION | QTY | UNIT | RATE | AMOUNT |
| A  B C  D  E  F  G  H  J  K  L  M N | BOUNDARY PALISADE FENCE  The following in wall and palisade boundary fence as described  Excavation works  Excavate over site average 150 mm deep to remove top soil and wheel, spread and level on site where directed.  Excavate for foundation trenches not exceeding 1.50metres deep, get out, part back fill and spread on site any surplus material as described  Extra over excavations for excavating in hard rock  Concrete works  Vibrated insitu concrete Grade 25 (20mm aggregate) as described in strip foundation  Vibrated insitu concrete Grade 25 (20mm aggregate) as described in isolated pads  Blockwork  Lay150 mm solid concrete blocks foundation walls, with cement mortar of ratio1:4;not more than1metre height blockwork from footing  Construct 150mm solid concrete block column size 400mm x 400mm x 2500m high from concrete pad, with cement mortar of ratio 1:4;  Lay 150 mm concrete blocks superstructure walls, with cement mortar of ratio 1:4- Area of blockwork for superstructure  Brick force reinforcement to wall joints every third course width 100mm end laps minimum 100mm wide  Pre-cast concrete (1:2: 4 - 20 mm aggregate as described, including all formwork, moulds, reinforcement, reinforcement for handling, hoisting in position, building in and bedding and pointing in cement mortar 1:4 as described  Concretecoping280mmx115mm(average) deep and bedding as described  Concretecoping500mmx115mm(average) deep and bedding as described  Wall Finishings  One coat wooden trowel finish cement sand (1:4) plaster: 15mm to dwarf walls  15mm to block column externally  Carried Forward | 200  240  24  60  16  250  126  250  1,000  500  63  500  373 | m²  m³m³  m³  m³  m²  nr  m²  m  m  m  m²m² |  | -  -  -  -  -  -  -  -  -  -  -  -  - |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ITEM | DESCRIPTION | QTY | UNIT | RATE | AMOUNT |
| A  B | Brought Forward  Painting and decorations  Plascon or equal and approved sealing coat, three coats AcrylicPVA paint as described to:  Plastered walls and columns  Palisade Fencing  Palisade fence consisting of 75 x75mm square hollow tube framing,30x30mm steel angles spaced at 150mm centres sharpened at the top end and 2 no.50x50mm square steel horizontal member anchored to block column withdrawal bolts  BOUNDARY FENCE -TOTALCARRIED TO GENERAL SUMMARY |  |  |  | - |
| 873 | m² |  | - |
| 810 | m² |  | - |
|  |  | K | - |

|  |  |  |  |
| --- | --- | --- | --- |
| ITEM | DESCRIPTION | PAGE | AMOUNT (ZMW) |
| AB C | MAIN SUMMARY |  |  |
| PRELIMINARY AND GENERAL ITEMS | 1/1 | - |
| DEMOLITIONS | 2/1 | - |
| PALISADE BOUNDARY FENCE | 2/3 | - |
| SUBTOTAL 1 |  | - |
| ADD 5% CONTIGENCY |  | - |
| SUBTOTAL 2 |  | - |
| ADD 16% VAT |  | - |
| TOTAL TENDER SUM |  | - |
| Name of Contractor: |  |  |
| Address: |  |
|  | Signature: |  |
| Date: |  |

**NB: All bidders have to mandatorily visit the site on 17 November 2023 at 10:00hours for them to qualify for bidding.**

**ANNEXURE C: THE CONTRACTOR’S BID AND ORIGINAL PRICE SCHEDULES**

**ANNEXURE D: THE CONTRACTOR’S BID AND ORIGINAL PRICE SCHEDULES**

**ANNEXURE E: THE CONTRACTING AUTHORITY’S NOTIFICATION OF AWARD**

**ANNEXURE F: Acceptance to Award of Contract**